1.Pull up pins of MCU XC2361 no.60 and 62.
2.Conect pull up pins 60 , 62  , red point and red wire of programmer like show on pic1.jpg
3.conect black wire like pic1.jpg
4.Conect points yellow, GRAY , blue  to programmer like on pic2.jpg
5.Conect external supply 12V to AirBag module like on pic3.jpg

The red wire is +5V and is output from programmer. Red color is show some time on pictures and all time is the 
same wire .
 ONLY on pic3.jpg the red wire is +12V and never conect it to +5V from programmer!!!!!!!!!!